A Big Earth Data Platform for Three Poles

**Supervisory monitoring results of sewage treatment plants in Zeku County, Gangcha County, Haiyan County, Qilian County, Henan County, Jianzha County and Tongren County (2020)**

1、Description

The data set records the supervisory monitoring results of sewage treatment plants in Zeku County, Gangcha County, Haiyan County, Qilian County, Henan County, Jianzha county and Tongren County (2020.1-2020.6). The data is collected from the Department of ecological environment of Qinghai Province. The data set contains seven documents, namely: supervisory monitoring of Gangcha sewage treatment plant in 2020.pdf, In 2020, Haiyan County sewage treatment plant of Haibei Prefecture was monitored.pdf; in 2020, Qilian sewage treatment plant was monitored.pdf; in the first half of 2020, Jianzha county sewage treatment plant was monitored; in the first half of 2020, Tongren County sewage treatment plant was monitored; in the first half of 2020, Zeku County sewage treatment plant was monitored; in the first half of 2020, Henan county sewage treatment plant was monitored The results of supervision monitoring. The data monitoring entrusted units are Zeku County, Gangcha County, Haiyan County, Qilian County, Henan County, Jianzha county and Tongren County Environmental Bureau;
Detection point: inlet and outlet of sewage treatment plant
Detection items: water temperature, flow rate, pH value, chromaticity, chemical oxygen demand, five-day biochemical oxygen demand, ammonia nitrogen, total phosphorus, total nitrogen, lead, cadmium, chromium, sclera, arsenic, suspended solids, hexavalent chromium, petroleum, animal and vegetable oil, anionic surfactant, fecal coliform, alkyl mercury, free chlorine (free residual chlorine), a total of 22 items
Detection frequency:
1. Water temperature, pH value and flow rate are sampled in 24h, measured on site, and measured once every 2h (the average value of data is measured);
2. Chemical oxygen demand powder, suspended solids, five-day biochemical oxygen demand, petroleum, animal and vegetable oil, fecal coliform group are sampled by 24h, once every 2h, and all items are collected and packed separately (the average value of data is determined)
3. The other 13 items were sampled every 2 hours and mixed samples were taken for 24 hours

2、Keywords

Theme：Industrial emissions,Environment Pollution and Control
Discipline：Human-nature Relationship
Places：Haiyan County, Jianzha County, Henan County, Zeku County, Gangcha County, Huangnan prefecture, Qilian County, Tongren County, Qinghai
Time：2020

3、Data details

1.Scale：None

2.Projection：None

3.Filesize：11.5MB

4.Data format：None

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：40.0 | - |
| west：89.0 | - | east：104.0 |
| - | south：31.0 | - |

5、Time frame:2019-12-31 16:00:00+00:00--2020-12-30 16:00:00+00:00

6、Reference method

References to data:

Department of Ecology and Environment of Qinghai Province. Supervisory monitoring results of sewage treatment plants in Zeku County, Gangcha County, Haiyan County, Qilian County, Henan County, Jianzha County and Tongren County (2020). A Big Earth Data Platform for Three Poles, 2021

References to articles:

7、Supporting project information

8、Data resource provider

name: Department of Ecology and Environment of Qinghai Province
unit:
email: zhaohu361@163.com