A Big Earth Data Platform for Three Poles

**WATER: Dataset of airborne LiDAR mission in the Dayekou flight zone on Jun. 20, 2008**

1、Description

The dataset of airborne LiDAR mission in the Dayekou flight zone on Jun. 20, 2008 included peak pulse data (\*.LAS), full waveform data (.lgc), CCD photos, DEM, DSM and DOM. The DEM, DSM and DOM data are stored along with the Dataset of airborne LiDAR mission in the Dayekou flight zone on Jun. 23, 2008. The flight routes were as follows:  
  
{|  
! flight route   
! startpoint lat  
! startpoint lon  
! endpoint lat  
! endpoint lon  
! altitude (m)  
! length (km)  
! photos  
|-  
| 1 || 38°32′05.38″ || 100°12′24.59″ || 38°29′32.76″ || 100°18′35.69″ || 3650 || 10.1 || 49  
|-  
| 2 || 38°32′11.13″ || 100°12′28.42″ || 38°29′42.06″ || 100°18′30.89″ || 3650 || 9.9 || 46  
|-  
| 3 || 38°32′16.88″ || 100°12′32.24″ || 38°29′47.81″ || 100°18′34.72″ || 3650 || 9.9 || 47  
|-  
| 4 || 38°32′22.63″ || 100°12′36.07″ || 38°29′56.20″ || 100°18′32.15″ || 3650 || 9.7 || 45  
|-  
| 5 || 38°32′28.38″ || 100°12′39.90″ || 38°30′02.62″ || 100°18′34.33″ || 3650 || 9.7 || 47  
|-  
| 6 || 38°32′37.44″ || 100°12′35.66″ || 38°30′10.63″ || 100°18′32.68″ || 3650 || 9.8 || 44  
|-  
| 7 || 38°32′46.50″ || 100°12′31.43″ || 38°30′19.72″ || 100°18′28.37″ || 3650 || 9.8 || 47  
|}

2、Keywords

Theme：Airborne laser radar,Remote Sensing Technology,CCD  
Discipline：Remote Sensing Technology  
Places：Heihe River Basin, Dayekou watershed foci experimental areas, Forest and Hydrology Experimental Areas  
Time：

3、Data details

1.Scale：None

2.Projection：4326

3.Filesize：9049.4MB

4.Data format：

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：38.75 | - |
| west：100.15 | - | east：100.5 |
| - | south：38.45 | - |

5、Time frame:2008-07-04 10:00:00+00:00--2008-07-04 16:00:00+00:00

6、Reference method

References to data:

FAN Fengyun, BAO Yunfei, ZHOU Mengwei, HE Qisheng, LI Shiming, CHI Hong, PANG Yong, MA Mingguo. WATER: Dataset of airborne LiDAR mission in the Dayekou flight zone on Jun. 20, 2008. A Big Earth Data Platform for Three Poles, doi:10.3972/water973.0221.db2013

References to articles:

刘清旺. 机载激光雷达森林参数估测方法研究. 北京: 中国林业科学研究院, 2009.  
  
Tian, X., Li, Z.Y., van der Tol C, Su, Z., Li, X., He, Q.S., Bao, Y.F., Chen, E.X., & Li, L.H. (2011). Estimating zero-plane displacement height and aerodynamic roughness length using synthesis of LiDAR and SPOT-5 data. Remote Sensing of Environment, 115(9): 2330-2341. 10.1016/j.rse.2011.04.033.  
  
Bao YF, Cao CX, Zhang H, Chen EX, He QS, Huang HB, Ll ZY, Ll XW, Gong P. Synchronous estimation of DTM and fractional vegetation cover in forested area from airborne LIDAR height and intensity data. Science in China Series E-technological Sciences, 2008, 52(Suppl. 2): 176-187. 10.1007/s11431-008-6018-x.

7、Supporting project information

The CAS (Chinese Academy of Sciences) Action Plan for West Development Project  
National Program on Key Basic Research Project (973 Program

8、Data resource provider

name: MA Mingguo  
unit: Cold and Arid Regions Environmental and Engineering Research Institute, Chinese Academy of Sciences  
email: mmg@lzb.ac.cn  
  
name: BAO Yunfei  
unit: Beijing Normal University  
email:   
  
name: HE Qisheng  
unit:   
email: hqsfei999@163.com  
  
name: CHI Hong  
unit:   
email:   
  
name: ZHOU Mengwei  
unit:   
email: mengweizhou@hotmail.com  
  
name: FAN Fengyun  
unit:   
email:   
  
name: PANG Yong  
unit:   
email:   
  
name: LI Shiming  
unit:   
email: