A Big Earth Data Platform for Three Poles

**HiWATER：Dataset of hydrometeorological observation network (automatic weather station of Huangcaogou station, 2015)**

1、Description

This data set contains meteorological element observation data from January 1, 2015 to April 17, 2015 from huangcaogou station, upstream of heihe hydrometeorological observation network.The station is located in huangcaogou village, ebao town, qilian county, qinghai province.The latitude and longitude of the observation point is 100.7312e, 38.0033n and 3137m above sea level.The air temperature and relative humidity sensors are located at 5m, facing due north.The barometer is installed in the anti-skid box on the ground;The tilting bucket rain gauge is installed at 10m;The wind speed and direction sensor is set at 10m, facing due north;The four-component radiometer is installed at 6m, facing due south;Two infrared thermometers are installed at 6m, facing due south, and the probe facing vertically downward;The soil temperature probe is buried at 0cm on the surface and 4cm underground, 10cm, 20cm, 40cm, 80cm, 120cm, 160cm, 2m to the south of the meteorological tower.The soil water probe is buried at 4cm, 10cm, 20cm, 40cm, 80cm, 120cm and 160cm underground, 2m to the south of the meteorological tower.The soil heat flow plates (3 pieces) are buried in the ground 6cm underground, 2m to the south of the meteorological tower.  
Observation projects are: air temperature and humidity (Ta\_5m, RH\_5m) (unit: c, percentage), pressure (Press) (unit: hundred mpa), precipitation (Rain) (unit: mm), wind speed (WS\_10m) (unit: m/s), wind (WD\_10m) (unit: degrees), the radiation of four component (DR, UR, DLR\_Cor, ULR\_Cor, Rn) (unit: watts per square meter), the surface radiation temperature (IRT\_1, IRT\_2) (unit:Soil heat flux (Gs\_1, Gs\_2, Gs\_3) (in watts/m2), soil temperature (Ts\_0cm, Ts\_4cm, Ts\_10cm, Ts\_20cm, Ts\_80cm, Ts\_120cm, Ts\_160cm) (in Celsius), soil moisture (Ms\_4cm, Ms\_10cm, Ms\_20cm, Ms\_40cm, Ms\_80cm, Ms\_120cm, Ms\_160cm) (unit: percentage).  
Processing and quality control of observed data :(1) ensure 144 pieces of data every day (every 10min), and mark by -6999 in case of data missing;(2) excluding the time with duplicate records;(3) data that obviously exceeds the physical significance or the range of the instrument is deleted;(4) the part marked with red letter in the data is the data in question, and there are many questions about the measured wind direction of the station;(5) date and time have the same format, and date and time are in the same column.For example, the time is: September 10, 2015, 10:30;(6) the naming rule is: AWS+ site name.The station was demolished after April 17.  
For information of hydrometeorological network or station, please refer to Li et al. (2013), and for observation data processing, please refer to Liu et al. (2011).

2、Keywords

Theme：Precipitation,Meteorological element  
Discipline：Atmosphere  
Places：Heihe River Basin, the cold region hydrology experimental area in the upper reaches, Huangcaogou station  
Time：2015, 2015-01-01 to 2015-12-31

3、Data details

1.Scale：None

2.Projection：4326

3.Filesize：4.79MB

4.Data format：文本

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：38.0033 | - |
| west：100.7312 | - | east：100.7312 |
| - | south：38.0033 | - |

5、Time frame:2015-07-16 16:00:00+00:00--2015-10-30 16:00:00+00:00

6、Reference method

References to data:

TAN Junlei, LI Xin, LIU Shaomin, XU Ziwei, CHE Tao, ZHANG Yang. HiWATER：Dataset of hydrometeorological observation network (automatic weather station of Huangcaogou station, 2015). A Big Earth Data Platform for Three Poles, doi:10.3972/hiwater.313.2016.db2017

References to articles:

Liu, S.M., Xu, Z.W., Wang, W.Z., Bai, J., Jia, Z., Zhu, M., & Wang, J.M. (2011). A comparison of eddy-covariance and large aperture scintillometer measurements with respect to the energy balance closure problem. Hydrology and Earth System Sciences, 15(4), 1291-1306.  
  
Che, T., Li, X., Liu, S., Li, H., Xu, Z., Tan, J., Zhang, Y., Ren, Z., Xiao, L., Deng, J., Jin, R., Ma, M., Wang, J., & Yang, X. (2019). Integrated hydrometeorological, snow and frozen-ground observations in the alpine region of the Heihe River Basin, China. Earth System Science Data, 11, 1483-1499  
  
Liu, S., Li, X., Xu, Z., Che, T., Xiao, Q., Ma, M., Liu, Q., Jin, R., Guo, J., Wang, L., Wang, W., Qi, Y., Li, H., Xu, T., Ran, Y., Hu, X., Shi, S., Zhu, Z., Tan, J., Zhang, Y., Ren, Z. (2018). The Heihe Integrated Observatory Network: A basin‐scale land surface processes observatory in China. Vadose Zone Journal, 17,180072. https://doi.org/10.2136/vzj2018.04.0072.

7、Supporting project information

8、Data resource provider

name: XU Ziwei  
unit: Beijing Normal University  
email: xuzw@bnu.edu.cn  
  
name: TAN Junlei  
unit:   
email: tanjunlei@163.com  
  
name: ZHANG Yang  
unit:   
email: zhangyang@lzb.ac.cn  
  
name: LI Xin  
unit:   
email: xinli@itpcas.ac.cn  
  
name: LIU Shaomin  
unit: Beijing Normal University  
email: smliu@bnu.edu.cn  
  
name: CHE Tao  
unit:   
email: chetao@lzb.ac.cn