A Big Earth Data Platform for Three Poles

**Multi-scale surface flux and meteorological elements observation dataset in the Haihe River Basin (Huailai station-lysimeters, 2015)**

1、Description

The data set contains the observation data of the evapotranspiration apparatus on January 1, 2015, solstice, December 31, 2015.The site is located in huailai county, hebei province, east garden town, the underlying surface for corn.The latitude and longitude of the observation point is 115.7880E, 40.3491N, and the altitude is 480m.  
The acquisition frequency of the evapotranspiration permeameter is 1Hz, and the released data is 10min output data.The evapotranspiration meter is a cylindrical structure with a surface area of 1m2 and a buried depth of 1.5m. The observation accuracy of evapotranspiration is 0.01mm.Two evapotranspiration seeptometers were installed, one kept bare soil (lysimeter\_1), the other for the corn underlay (lysimeter\_2) during the growing season (May 10 - September 15).Soil temperature and humidity probe, soil water potential probe and soil heat flow plate are also installed in the evapotranspiration apparatus.The buried depth of the soil temperature sensor is 5cm, 30cm, 50cm, 100cm and 140cm.The buried depth of the soil water sensor is 2cm, 10cm, 20cm and 40cm.The soil heat flux plate is buried 10cm underground;The buried depth of the soil water potential sensor was 30cm and 140cm.Processing and quality control of observation data :(1) ensure 144 data per day (every 10min). If data is missing, it will be marked by -6999;Due to instruments and weather, the data was abnormal from December 6th to 31st.(2) delete the data of observation anomalies caused during maintenance;(3) data that is obviously beyond the physical meaning or the range of the instrument is deleted;(4) the format of date and time is unified, and the date and time are in the same column.For example, the time is: 10:30 on June 10, 2015.  
The observation data released by the evapotranspiration permeameter include:Date/Time, weighing mass (i.l.\_1\_wag\_l\_000 (Kg), i.l.\_2\_wag\_l\_000 (Kg)), seepage mass (i.l.\_1\_wag\_d\_000 (Kg), i.l.\_2\_wag\_d\_000 (Kg)), soil heat flux (Gs\_1\_10cm, Gs\_2\_10cm) (W/m2),Multi-layer soil moisture (Ms\_1\_5cm, Ms\_1\_10cm, Ms\_1\_30cm, Ms\_1\_50cm, Ms\_1\_50cm, Ms\_1\_100cm, Ms\_2\_5cm, Ms\_2\_10cm, Ms\_2\_30cm, Ms\_2\_50cm, Ms\_2\_100cm) (%),Multi-layer soil temperature (Ts\_1\_5cm, Ts\_1\_30cm, Ts\_1\_50cm, Ts\_1\_100cm, Ts\_1\_140cm, Ts\_2\_140cm, ts\_2\_2\_5cm, ts\_2\_2\_50cm, Ts\_2\_100cm, Ts\_2\_140cm) (℃), soil water potential (TS\_1\_30 (hPa), TS\_1\_140 (hPa), TS\_2\_30 (hPa), TS\_2\_30 (hPa), TS\_2\_140 (hPa), TS\_2\_140 (hPa));The data is stored in \*.xls format.  
Please refer to Liu et al. (2013) for information of observation test or site, and Yang guangchao et al. (2015) for data processing.

2、Keywords

Theme：Soil,Lysimeter,Soil moisture/Water content,Soil heat flux  
Discipline：Atmosphere,Terrestrial Surface  
Places：Huailai, Hebei, Haihe river basin  
Time：2015

3、Data details

1.Scale：None

2.Projection：None

3.Filesize：2.6MB

4.Data format：EXCEL

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：40.3491 | - |
| west：115.788 | - | east：115.788 |
| - | south：40.3491 | - |

5、Time frame:2015-01-10 00:00:00+00:00--2016-01-09 00:00:00+00:00

6、Reference method

References to data:

LIU Shaomin, XU Ziwei, ZHU Zhongli, XIAO Qing. Multi-scale surface flux and meteorological elements observation dataset in the Haihe River Basin (Huailai station-lysimeters, 2015). A Big Earth Data Platform for Three Poles, doi:10.3972/haihe.020.2016.db2016

References to articles:

Liu, S.M., Xu, Z.W., Zhu, Z.L., Jia, Z.Z., & Zhu, M.J. (2013). Measurements of evapotranspiration from eddy-covariance systems and large aperture scintillometers in the Hai River Basin, China. Journal of Hydrology, 487, 24-38.  
  
杨光超, 朱忠礼, 谭磊, 刘绍民, 徐自为, 柏军华, 肖青. (2015). 怀来地区蒸渗仪测定玉米田蒸散发分析. 高原气象, 34(4), 1095-1106.

7、Supporting project information

8、Data resource provider

name: ZHU Zhongli  
unit:   
email: zhuzl@bnu.edu.cn  
  
name: XU Ziwei  
unit: Beijing Normal University  
email: xuzw@bnu.edu.cn  
  
name: XIAO Qing  
unit: Institute of Remote Sensing and Digital Earth, Chinese Academy of Sciences  
email: xiaoqing@irsa.ac.cn  
  
name: LIU Shaomin  
unit: Beijing Normal University  
email: smliu@bnu.edu.cn