A Big Earth Data Platform for Three Poles

**Qilian Mountains integrated observatory network: Dataset of Heihe integrated observatory network (automatic weather station of mixed forest station, 2021)**

1、Description

This dataset includes data recorded by the Heihe integrated observatory network obtained from the automatic weather station (AWS) at the Sidaoqiao mixed forest station from January 1 to December 31, 2021. The site (101.134° E, 41.990° N) was located on a tamarix and populous forest (Tamarix chinensis Lour. and Populus euphratica Olivier.) surface in the Sidaoqiao, Dalaihubu Town, Ejin Banner, Inner Mongolia Autonomous Region. The elevation is 874 m. The installation heights and orientations of different sensors and measured quantities were as follows: air temperature and humidity profile (28 m, north), wind speed and direction profile (28 m, north), air pressure (in tamper box), rain gauge (28 m, south), four-component radiometer (24 m, south), two infrared temperature sensors (24 m, south, vertically downward), two photosynthetically active radiation (24 m, south, one vertically upward and one vertically downward), soil heat flux (HFP01; 3 duplicates, -0.06 m), soil temperature profile (0, -0.02, -0.04, -0.1, -0.2, -0.4, -0.6, -1.0, -1.6, -2.0, -2.4 m), and soil moisture profile (-0.02, -0.04, -0.1, -0.2, -0.4, -0.6, -1.0, -1.6, -2.0, -2.4 m).  
The observations included the following: air temperature and humidity (Ta\_28 m; RH\_28 m) (℃ and %, respectively), wind speed (Ws\_28 m) (m/s), wind direction (WD\_28 m) (°), air pressure (press) (hpa), precipitation (rain) (mm), four-component radiation (DR, incoming shortwave radiation; UR, outgoing shortwave radiation; DLR\_Cor, incoming longwave radiation; ULR\_Cor, outgoing longwave radiation; Rn, net radiation) (W/m^2), infrared temperature (IRT\_1 and IRT\_2) (℃), photosynthetically active radiation of upward and downward (PAR\_up and PAR\_down) (μmol/ (s m^-2)), soil heat flux (Gs\_1, Gs\_2 and Gs\_3) (W/m^2), soil temperature (Ts\_0 cm, Ts\_2 cm, Ts\_4 cm, Ts\_20 cm, Ts\_40 cm, Ts\_60 cm, Ts\_100, Ts\_160, Ts\_200, Ts\_240 cm) (℃), and soil moisture (Ms\_2 cm, Ms\_4 cm, Ms\_10 cm, Ms\_20 cm, Ms\_40 cm, Ms\_60 cm, Ms\_100, Ms\_160, Ms\_200, Ms\_240 cm) (%, volumetric water content).  
The data processing and quality control steps were as follows: (1) The AWS data were averaged over intervals of 10 min for a total of 144 records per day. The missing data were denoted by -6999. (2) Data in duplicate records were rejected. (3) Unphysical data were rejected. (4) The data marked in red are problematic data. (5) The format of the date and time was unified, and the date and time were collected in the same column, for example, date and time: 2019-9-10 10:30. (6) Finally, the naming convention was AWS+ site no. Moreover, suspicious data were marked in red.  
For more information, please refer to Liu et al. (2018) (for sites information), Liu et al. (2011) for data processing) in the Citation section.

2、Keywords

Theme：Visibility,Hydrology  
Discipline：Atmosphere,Terrestrial Surface  
Places：The lower reaches of the heihe river, mixed forest station, Heihe River Basin  
Time：2021

3、Data details

1.Scale：None

2.Projection：

3.Filesize：13.6MB

4.Data format：None

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：41.9903 | - |
| west：101.1335 | - | east：101.1335 |
| - | south：41.9903 | - |

5、Time frame:2020-12-31 16:00:00+00:00--2021-12-31 03:59:59+00:00

6、Reference method

References to data:

LIU Shaomin, ZHANG Yang, XU Ziwei, REN Zhiguo, TAN Junlei, CHE Tao. Qilian Mountains integrated observatory network: Dataset of Heihe integrated observatory network (automatic weather station of mixed forest station, 2021). A Big Earth Data Platform for Three Poles, doi:10.11888/Atmos.tpdc.2724892022

References to articles:

Liu, S.M., Xu, Z.W., Wang, W.Z., Bai, J., Jia, Z., Zhu, M., & Wang, J.M. (2011). A comparison of eddy-covariance and large aperture scintillometer measurements with respect to the energy balance closure problem. Hydrology and Earth System Sciences, 15(4), 1291-1306.  
  
Liu, S.M., Li, X., Xu, Z.W., Che, T., Xiao, Q., Ma, M.G., Liu, Q.H., Jin, R., Guo, J.W., Wang, L.X., Wang, W.Z., Qi, Y., Li, H.Y., Xu, T.R., Ran, Y.H., Hu, X.L., Shi, S.J., Zhu, Z.L., Tan, J.L., Zhang, Y., & Ren, Z.G. (2018). The Heihe Integrated Observatory Network: A Basin-Scale Land Surface Processes Observatory in China. Vadose Zone Journal, 17(1), 180072.

7、Supporting project information

Pan-Third Pole Environment Study for a Green Silk Road-A CAS Strategic Priority A Program

8、Data resource provider

name: XU Ziwei  
unit: Beijing Normal University  
email: xuzw@bnu.edu.cn  
  
name: LIU Shaomin  
unit: Beijing Normal University  
email: smliu@bnu.edu.cn  
  
name: CHE Tao  
unit:   
email: chetao@lzb.ac.cn  
  
name: ZHANG Yang  
unit:   
email: zhangyang@lzb.ac.cn  
  
name: TAN Junlei  
unit:   
email: tanjunlei@lzb.ac.cn  
  
name: REN Zhiguo  
unit:   
email: rzgehu@lzb.ac.cn