A Big Earth Data Platform for Three Poles

**WATER: Dataset of ground truth measurements synchronizing with Envisat ASAR in the Linze grassland foci experimental area on Jul. 11, 2008**

1、Description

The dataset of ground truth measurements synchronizing with Envisat ASAR was obtained in the Linze grassland foci experimental area on Jul. 11, 2008.
 The data were in AP mode and VV/VH polarization combinations, and the overpass time was approximately at 11:26 BJT. Observations were carried out in the reed plot A, the saline plots B and C, the alfalfa plot D and the barley plot E, which were divided into 6×6 subsites, with each one spanning a 120×120 m2 plot. Soil gravimetric moisture, volumetric moisture, and soil bulk density after drying by using the cutting ring, the mean soil temperature from 0-5cm by the probe thermometer, and the canopy temperature and the land surface temperature by the hand-held infrared thermometer were measured in A, B and C; the soil temperature, soil moisture, the loss tangent, soil conductivity, the real part and the imaginary part of soil complex permittivity by the POGO soil sensor, the mean soil temperature from 0-5cm by the probe thermometer, the canopy temperature and the land surface temperature by the hand-held infrared thermometer in D and E.
 Data were archived in Excel file. See WATER: Dataset of setting of the sampling plots and stripes in the foci experimental area of Linze station for more information.

2、Keywords

Theme：Soil,Surface radiation temperature,Vegetation,Earth SurFace Processes,Soil temperature,Canopy temperature,Soil moisture/Water content,Terrestrial Surface Remote Sensing,Ground verification information
Discipline：Terrestrial Surface
Places：Heihe River Basin, Arid Region Hydrology in the Middle Reaches,
Time：2008,

3、Data details

1.Scale：None

2.Projection：4326

3.Filesize：692.7MB

4.Data format：EXCEL

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：39.268 | - |
| west：100.037 | - | east：100.095 |
| - | south：39.225 | - |

5、Time frame:2008-07-22 08:00:00+00:00--2008-07-22 08:00:00+00:00

6、Reference method

References to data:

WU Yueru, GE Chunmei. WATER: Dataset of ground truth measurements synchronizing with Envisat ASAR in the Linze grassland foci experimental area on Jul. 11, 2008. A Big Earth Data Platform for Three Poles, doi:10.3972/water973.0074.db2013

References to articles:

7、Supporting project information

The CAS (Chinese Academy of Sciences) Action Plan for West Development Project
National Program on Key Basic Research Project (973 Program

8、Data resource provider

name: GE Chunmei
unit: Cold and Arid Regions Environmental and Engineering Research Institute, Chinese Academy of Sciences
email: gechm@lzb.ac.cn

name: WU Yueru
unit:
email: