A Big Earth Data Platform for Three Poles

**HiWATER: Dataset of hydrometeorological observation network (No.6 runoff observation system of Gaoya hydrological station, 2014)**

1、Description

The data set includes the observation data of river water level and velocity at No. 6 point in the dense observation of runoff in the middle reaches of Heihe River from January 1, 2014 to December 31, 2014. The observation point is located in Gaoya National Hydrological Station, zhaojiatunzhuang, Ganzhou District, Zhangye City, Gansu Province. The riverbed is sandy gravel with stable section. The longitude and latitude of the observation point are n39 ° 08'06.35 ", E100 ° 25'58.23", 1420 m above sea level, and 50 m wide river channel. Hobo pressure water level gauge is used for water level observation, with acquisition frequency of 60 minutes. Data description includes the following two parts:  
Water level observation, 60 minutes in unit (cm) in 2014; Data covers the period of January 1, 2014 solstice December 31, 2014; Flow observation, unit (m3); According to the monitoring flow of different water levels, the flow curve of water levels was obtained, and the change process of runoff was obtained by observing the process of water levels.The missing data are uniformly represented by the string -6999.  
For information of hydrometeorological network or station, please refer to Li et al.(2013), and for observation data processing, please refer to He et al.(2016).

2、Keywords

Theme：Surface Water,Hydrology section,Discharge/Flow,Runoff  
Discipline：Terrestrial Surface  
Places：Heihe River Basin, the artificial oasis experimental area in the middle reaches,   
Time：2014, 2014-01-01 to 2014-12-31

3、Data details

1.Scale：None

2.Projection：4326

3.Filesize：0.66MB

4.Data format：EXCEL

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：39.135 | - |
| west：100.398333 | - | east：100.398889 |
| - | south：39.134722 | - |

5、Time frame:2014-01-09 16:00:00+00:00--2015-01-08 16:00:00+00:00

6、Reference method

References to data:

LI Xin, LIU Shaomin, XU Ziwei, HE Xiaobo. HiWATER: Dataset of hydrometeorological observation network (No.6 runoff observation system of Gaoya hydrological station, 2014). A Big Earth Data Platform for Three Poles, doi:10.3972/hiwater.231.2015.db2016

References to articles:

Li X, Cheng GD, Liu SM, Xiao Q, Ma MG, Jin R, Che T, Liu QH, Wang WZ, Qi Y, Wen JG, Li HY, Zhu GF, Guo JW, Ran YH, Wang SG, Zhu ZL, Zhou J, Hu XL, Xu ZW. Heihe Watershed Allied Telemetry Experimental Research (HiWATER): Scientific objectives and experimental design. Bulletin of the American Meteorological Society, 2013, 94(8): 1145-1160, 10.1175/BAMS-D-12-00154.1.  
  
Liu, S.M., Li, X., Xu, Z.W., Che, T., Xiao, Q., Ma, M.G., Liu, Q.H., Jin, R., Guo, J.W., Wang, L.X., Wang, W.Z., Qi, Y., Li, H.Y., Xu, T.R., Ran, Y.H., Hu, X.L., Shi, S.J., Zhu, Z.L., Tan, J.L., Zhang, Y., & Ren, Z.G. (2018). The Heihe Integrated Observatory Network: A Basin-Scale Land Surface Processes Observatory in China. Vadose Zone Journal, 17(1), 180072. doi:10.2136/vzj2018.04.0072.

7、Supporting project information

National Natural Science Foundation of China

8、Data resource provider

name: XU Ziwei  
unit: Beijing Normal University  
email: xuzw@bnu.edu.cn  
  
name: HE Xiaobo  
unit: Cold and Arid Regions Environmental and Engineering Research Institute, Chinese Academy of Sciences  
email: hxb@lzb.ac.cn  
  
name: LI Xin  
unit:   
email: xinli@itpcas.ac.cn  
  
name: LIU Shaomin  
unit: Beijing Normal University  
email: smliu@bnu.edu.cn