A Big Earth Data Platform for Three Poles

**Integrated remote sensing experiment of Heihe River: ENVISAT AATSR remote sensing data set**

1、Description

Advanced along orbit scanning radiometer (AATSR) is an advanced tracking scanning radiometer sensor mounted on the European Space Agency ENVISAT satellite. It is one of many high-precision and stable infrared radiometers for retrieving sea surface temperature (SST). Its accuracy can reach 0.3k, and it can also be used to record meteorological data. AATSR is a multi-channel imaging radiometer. Its main goal is to provide global ocean surface temperature with high accuracy and stability for monitoring the earth's climate change. At present, there are 38 ENVISAT AATSR images in Heihe River Basin.   
The acquisition time is 2008-05-17 (2 scenes), 2008-05-27 (2 scenes), 2008-05-30 (2 scenes), 2008-06-02 (2 scenes), 2008-06-12 (2 scenes), 2008-06-15 (2 scenes), 2008-06-18 (2 scenes), 2008-06-21 (2 scenes), 2008-07-04 (2 scenes), 2008-07-072008-07-102008-07-172008-07-202008-07-232008-07-262008-08-022008-08-052008-08-082008 -08-11，2008-08-14，2008-08-21，2008-08-24，2008-08-27，2008-08-30，2008-09-06，2008-09-12，2008-09-15，2008-09-18，2008-09-25。   
The product level is L1B, which has been corrected by radiation but not by geometry.   
The ENVISAT AATSR remote sensing data set of Heihe comprehensive remote sensing joint test was obtained through the China EU "dragon plan" project (Project No.: 5322) (see the data use statement for details).

2、Keywords

Theme：Remote Sensing Technology,Visible remote sensing  
Discipline：Remote Sensing Technology  
Places：Heihe River Basin, Forest and Hydrology Experimental Areas, Arid Region Hydrology in the Middle Reaches, the cold region hydrology experimental area in the upper reaches  
Time：2008.05-2008.09

3、Data details

1.Scale：None

2.Projection：4326

3.Filesize：29572.3MB

4.Data format：

4、Space scope

|  |  |  |
| --- | --- | --- |
| - | north：42.685 | - |
| west：97.399 | - | east：102.125 |
| - | south：37.683 | - |

5、Time frame:2008-05-26 16:20:00+00:00--2008-10-04 16:20:00+00:00

6、Reference method

References to data:

LI Xin. Integrated remote sensing experiment of Heihe River: ENVISAT AATSR remote sensing data set. A Big Earth Data Platform for Three Poles, 2011

References to articles:

7、Supporting project information

The CAS (Chinese Academy of Sciences) Action Plan for West Development Project  
National Program on Key Basic Research Project (973 Program

8、Data resource provider

name: LI Xin  
unit:   
email: xinli@itpcas.ac.cn