时空三极环境大数据平台

**A long term half-hourly eddy covariance dataset of consistently processed CO2 and H2O Fluxes from the Tibetan Alpine Steppe at Nam Co (2005 - 2019)**

英文标题：A long term hourly eddy covariance dataset of consistently processed CO2 and H2O Fluxes from the Tibetan Alpine Steppe at Nam Co (2005 - 2019)

1、摘要

The data set contains nearly 15 years of eddy covariance data from an alpine steppe ecosystem on the central Tibetan Plateau.The data was processed following standardized quality control methods to allow for comparability between the different years of our record and with other data sets. To ensure meaningful estimates of ecosystem atmosphere exchange, careful application of the following correction procedures and analyses was necessary: (1) Due to the remote location, continuous maintenance of the eddy covariance (EC) system was not always possible, so that cleaning and calibration of the sensors was performed irregularly. Furthermore, the high proportion of bare soil and high wind speeds led to accumulation of dirt in the measurement path of the infrared gas analyzer (IRGA). The installation of the sensor in such a challenging environment resulted in a considerable drift in CO2 and H2O gas density measurements. If not accounted for, this concentration bias may distort the estimation of the carbon uptake. We applied a modified drift correction procedure following Fratini et al. (2014) which, instead of a linear interpolation between calibration dates, uses the CO2 concentration measurements from the Mt. Waliguan atmospheric observatory as reference time series. (2) We applied rigorous quality filtering of the calculated fluxes to retain only fluxes which represent actual physical processes. (3) During the long measurement period, there were several buildings constructed in the near vicinity of the EC system. We investigated the influence of these obstacles on the turbulent flow regime to identify fluxes with uncertain land cover contribution and exclude them from subsequent computations. (4) We calculated the de-facto standard correction for instrument surface heating during cold conditions (hereafter called sensor self heating correction) following Burba et al. (2008) and a revision of the original method following Frank and Massman (2020). (5)Subsequently, we applied the traditional and widely used gap filling procedure following Reichstein et al. (2005) to provide a more complete overview of the annual net ecosystem CO2 exchange.(6) We estimated the flux uncertainty by calculating the random flux error (RE) following Finkelstein and Sims (2001) and by using the standard deviation of the fluxes used for gap filling(NEE\_fsd) as a measure for spatial and temporal variation.

2、关键词

主题关键词：潜热通量,辐射,二氧化碳通量,感热通量  
学科关键词：大气  
地点关键词：Nam Co, Tibetan Plateau  
时间关键词：time series

3、数据细节

1.比例尺：None

2.投影：

3.文件大小：250.0MB

4.数据格式：None

4、空间范围

|  |  |  |
| --- | --- | --- |
| - | 北：30.772766 | - |
| 西：90.963043 | - | 东：90.963043 |
| - | 南：30.772766 | - |

5、时间范围2005-12-09 08:00:00+00:00--2019-09-12 08:00:00+00:00

6、引用方式

数据的引用:

Felix Nieberding, 马耀明, Christian Wille, Gerardo Fratini, Magnus Ole Asmussen, 王玉阳, 马伟强, Torsten Sachs. A long term half-hourly eddy covariance dataset of consistently processed CO2 and H2O Fluxes from the Tibetan Alpine Steppe at Nam Co (2005 - 2019). 时空三极环境大数据平台, DOI:10.11888/Meteoro.tpdc.270333, CSTR:18406.11.Meteoro.tpdc.270333, 2020.[Felix Nieberding, Yuyang Wang\*, MA Weiqiang\*, Torsten Sachs, MA Yaoming, Gerardo Fratini, Magnus Ole Asmussen, Cristian Wille. A long term hourly eddy covariance dataset of consistently processed CO2 and H2O Fluxes from the Tibetan Alpine Steppe at Nam Co (2005 - 2019). A Big Earth Data Platform for Three Poles, DOI:10.11888/Meteoro.tpdc.270333, CSTR:18406.11.Meteoro.tpdc.270333, 2020]

文章的引用:

Ma, Y.M., Kang, S.C., Zhu, L.P., Xu, B.Q., Tian, L.D., & Yao, T.D. (2008). Tibetan Observation and Research Platform- Atmosphere–land interaction over a heterogeneous landscape, Bulletin of the American Meteorological Society. 89, 1487–1492. doi:10.1175/2008BAMS2545.1.  
  
Ma, Y.M., Ma, W.Q., Zhong, L., Hu, Z., Li, M., Zhu, Z., et al. (2017). Monitoring and Modeling the Tibetan Plateau’s climate system and its impact on East Asia, Scientific Reports, 7, 44574, doi:10.1038/srep44574.  
  
Nieberding, F., Wille, C., Fratini, G., Asmussen, M. O., Wang, Y., Ma, Y., & Sachs, T. (2020). A long-term (2005–2019) eddy covariance data set of CO2 and H2O fluxes from the Tibetan alpine steppe. Earth System Science Data. 12. 2705-2724. 10.5194/essd-12-2705-2020.

7、资助项目信息

泛第三极环境变化与绿色丝绸之路建设专项  
第二次青藏高原综合科学考察研究

8、数据资源提供者

姓名: Felix Nieberding  
单位: Institute of Geosystems and Bioindication, Technische Universität Braunschweig, Germany  
电子邮件: felix.nieberding@posteo.de  
  
姓名: 马耀明  
单位: 中国科学院青藏高原研究所  
电子邮件: ymma@itpcas.ac.cn  
  
姓名: Christian Wille  
单位: GFZ German Research Centre for Geosciences, Potsdam, Germany  
电子邮件: christian.wille@gfz-potsdam.de  
  
姓名: Gerardo Fratini  
单位: LI-COR Biosciences Inc., Lincoln, Nebraska, USA  
电子邮件: gerardo.fratini@licor.com  
  
姓名: Magnus Ole Asmussen  
单位: Technische Universität Braunschweig, Germany  
电子邮件: m.asmussen@tu-braunschweig.de  
  
姓名: 王玉阳  
单位: deguo  
电子邮件: wangyuyang@itpcas.ac.cn  
  
姓名: 马伟强  
单位: 中国科学院青藏高原研究所  
电子邮件: wqma@itpcas.ac.cn  
  
姓名: Torsten Sachs  
单位: GFZ German Research Centre for Geosciences, Potsdam, Germany  
电子邮件: torsten.sachs@gfz-potsdam.de